Alamance County 
Residential Plan Review Requirements

The following is provided as a guide for obtaining Building plan approval for residential single-family dwellings, modular homes, and additions and renovations in Alamance County. 
It applies to all plans submitted under the 2018 NC Residential code.
· General
· All plans submitted for plan review must be submitted to planreview@alamance-nc.com 
· Plans must be submitted as one file in PDF format
· Floor plan layout with all rooms / areas labeled for use
· Window and door sizes
· Site plan 
· Insulation
· Insulation values for floors, walls and ceilings. Provide detail for monolithic slab foundations
· Structural  
· Footing and foundation details
· Thickened slab details for poured concrete foundations 
· Complete details for floor joists and girders for all floor systems 
· Sealed floor truss plans if they are used 
· Wall construction details, including stud height, size, spacing and wall bracing method / details
· We are no longer requiring roof truss drawings at plan review time, these should be placed in the permit box for the framing inspection. A layout is required as well
· If roof is stick framed, complete roof structural including - size, spacing, direction of all members including ceiling joists and all rafters
· All header and girder sizes with bearing and attachment details and locations (For LVL headers, the plans should just state ”LVL header”)
· The cut sheets for each LVL header must be in the permit box at the time of framing inspection.
· Point loaded LVL headers- cut sheet must be sealed by engineer
· Any steel girders must be sized and sealed by engineer
· Decks 
· Dimensional plans including: 
· Footings
· Post locations
· Girder and joist size, span, spacing and direction  
· Fire protection - duplex, townhome, multi-family
· Separation wall design and details
· Fire separation details for soffit

